
**Split 9 Patch – Tumbling Block Variation – 51 x 64 Finished**


**Requirements for Top**


* 10 (10”) Blocks – leftover layer cakes or 30” fabric
* 50 (5”) Print squares – leftover charms or 30” fabric
* 40 (5”) Solid (or Tone on Tone) squares – 25” fabric
* 5 (2 ½” ) Solid Strips subcut – 20 x 10” – 12 ½” fabric
* 8 (2 ½ ”) Solid Strips subcut – 20 x 14” – 20” fabric
* Total Solid fabric = 58” or 1.5m
* Binding – 6 (2 ½”) strips

**Split 9 Patch**

|  |  |  |
| --- | --- | --- |
| Print | Solid | Print |
| Solid | Print | Solid |
| Print | Solid | Print |







* Assemble 5” Print & Solids Blocks
* Cut in ½ in both directions to make 4 quarters



* Flip top left ¼ & bottom right ¼
* Reassemble to form chain link – approx. 13 ½” square

**10” Blocks**

* Sash sides using 10” strips
* Sash top & bottom using 14” strips
* Trim to approx. 13 ½” or size to match finished split 9 patches

SK Baldry 2019

|  |  |  |  |
| --- | --- | --- | --- |
| **10”**  **Block** | **Split 9** | **10”**  **Block** | **Split 9** |
| **Split 9** | **10”**  **Block** | **Split 9** | **10”**  **Block** |
| **10”**  **Block** | **Split 9** | **10”**  **Block** | **Split 9** |
| **Split 9** | **10”**  **Block** | **Split 9** | **10”**  **Block** |
| **10”**  **Block** | **Split 9** | **10”**  **Block** | **Split 9** |

